The Rapp Firm · Northern California Territory · AVPro Global Universe

# Roll Ready

Field Kit Essentials · Every SKU Verified · 2026 AVPro Edge Product Guide

Real product numbers. Real MSRPs. Real use cases from the field. These are the AVPro Edge universe products that earn their place behind the seats — the ones that turn a return trip into a closed ticket.

40+
Verified SKUs
7
Categories
10yr
No-BS Warranty
∞
Return Trips Avoided
Kit: 0 items
⚡ Field Scenarios
Problem → Product. No guessing.
The Dispatcher

Every service call maps to a product. Know the scenario, grab the box, close the ticket. These are the most common field problems and the AVPro tools that fix them on the first visit.

EDID / Handshake
"The source won't output 4K on this display"
Snap the AC-EDID-X (Contact RSM) between source and display. Override EDID, force the resolution. 30 seconds, done.
AVR Bypass
"My AVR doesn't support 4K60 but the TV does"
AC-MX-42 (Contact RSM) — Out 1 delivers full 18Gbps to the display. Out 2 downscales to 1080p into the legacy AVR. Video reduced, audio untouched.
eARC / ARC
"TV audio won't come through the sound system"
AC-AEX-DEARC-KIT (Contact RSM) extends eARC to 100m. Or AC-DAC-CO2 (Contact RSM) converts SPDIF to analog.
Legacy Cat Run
"The in-wall run has splices and punch-downs"
AC-EX150-BKT (Contact RSM) — built for retro installs with splices, couplers, and punch-down blocks. 100m 4K60, 150m 1080p over legacy Cat5e.
Dante Bridging
"Need to bridge this zone to the Dante network"
AC-DANTE-E + AC-DANTE-D (Contact RSM) — bridge any HDMI audio source onto the Dante fabric or pull Dante to any analog output.
USB / Conferencing
"Zoom camera won't work 70 feet from the room"
AC-EXUSB-3-KIT (Contact RSM) — USB 3.2 Gen 1 over Cat6a to 100m. Verified: Zoom, Teams, Logitech BRIO.
Audio Downmix
"Atmos/DTS:X won't downmix for the zone amp"
AC-AVDM-V3 (Contact RSM) — 8-channel bitstream downmixer, full Dolby Atmos and DTS:X. Referenced in the AC-MX-42 manual.
Signal Verification
"Does this display actually support Dolby Vision?"
MU-STIX-G + MU-STIX-A (Contact RSM) — pocket generator/analyzer. Inject test signals, read EDID and HDR capability at the display.
Conference Room
"HDMI vs USB-C — two different users every day"
AC-MX-42 auto-switching (Contact RSM) — enable auto mode, switches to last hot-plugged device. No button press, no programming.
TAA / Government
"GSA Schedule job — client requires TAA compliance"
AVPro is one of the few US manufacturers with declared TAA compliance. AC-EX70-444-KIT-TAA (Contact RSM), AC-EX40-444-KIT-TAA (Contact RSM), MXnet 1G TAA units.
🔑 EDID & Signal Management
Most service calls are EDID calls in disguise

The AC-EDID-X at Contact RSM is the most undercarried tool in the industry. Every HDMI handshake failure, every source that "won't output 4K," every display that ignores HDR — start here. It's 48Gbps capable and fits in a shirt pocket. Carry three.

AVPro Edge
AC-EDID-X Contact RSM
Compact 48Gbps HDMI EDID Manager

At Contact RSM there is zero excuse not to have three of these. Clamp between source and display to override EDID negotiation — force resolution, control audio formats, bypass broken display EDID entirely.

EDID
Must Carry ×3
AVPro Edge
AC-SC-1X Contact RSM
8K/40Gbps Down Scaler · EDID Manager · Audio De-Embedder

Three tools in one box: scales 8K/4K to any output resolution, manages EDID independently, and de-embeds audio to optical or analog. When the AC-EDID-X isn't enough.

EDID Scaler
Must Carry
AVPro Edge
AC-DA12-AUHD-GEN2 Contact RSM
1×2 18Gbps DA · Audio De-Embedding · Downscaling

The van workhorse. Split one source to two displays and test each path independently. Built-in audio de-embedding and downscaling — 4K HDR to the main display, scaled to legacy on Out 2. Simultaneously.

1×2 DA
Must Carry
AVPro Edge
AC-DA14-AUHD-GEN2 Contact RSM
1×4 18Gbps Distribution Amp · 4K60 4:4:4 HDR

Four independent outputs for staging multi-display zones, isolating the bad display, or covering when the matrix isn't on the truck. Test all four simultaneously.

1×4 DA
Must Carry
AVPro Edge
AC-DA-12X2 Contact RSM
1×2 48Gbps Distribution Amp · HDMI 2.1 · 8K Ready

The 48Gbps version for HDMI 2.1 installs. When the client has 4K/120Hz or 8K displays, the 18Gbps DA throttles the signal. Same Contact RSM full bandwidth. Carry alongside the GEN2.

48Gbps HDMI 2.1
Recommended
🔀 Matrix & Switching
Route anything, bypass the AVR, auto-switch the conference room
AVPro Edge
AC-MX-42 Contact RSM
4×2 18Gbps Auto-Switching Matrix · AVR Bypass · C4/RTI/ELAN/Crestron

The van matrix. Out 1: full 18Gbps to the display. Out 2: downscaled to 1080p for the legacy AVR — video reduced, audio untouched. Conference room auto-switching on hot-plug. Web GUI at 192.168.1.239. Toslink + balanced analog audio extraction built in.

4×2 AVR Bypass Auto-Switch
Must Carry
AVPro Edge
AC-MX-42X Contact RSM
4×2 40Gbps 8K HDMI 2.1 Matrix · Per-Output Downscaling

The HDMI 2.1 version. 8K/60Hz, 4K/144Hz, VRR, ALLM, Dolby Vision. Per-output downscaling for legacy displays. The swap-in spare when the installed unit is HDMI 2.1.

4×2 HDMI 2.1 8K
Recommended
AVPro Edge
AC-CX42-AUHD Contact RSM
ConferX 4×2 18Gbps HDMI/HDBaseT Conference Matrix · HDCP 2.3

Conference-room-specific matrix with HDBaseT I/O, advanced EDID management, and multi-format auto-sensing. When a conference room is down, this matches the installed feature set and form factor.

ConferX HDBaseT
Recommended
AVPro Edge
AC-AVDM-V3 Contact RSM
18Gbps 8-Channel Bitstream Audio Downmixer · Dolby Atmos · DTS:X

The Atmos/DTS:X-to-stereo bridge. When matrix audio extraction sends a full bitstream to a zone amp that only takes 2CH PCM. Referenced in the AC-MX-42 manual for combination systems.

Atmos DTS:X Downmix
Recommended
📡 Extension
HDBaseT, fiber, and the new hero for legacy runs
New: AC-EX150-BKT — The Retro Run Rescue · Contact RSM

Engineered specifically for retro installs with splices, couplers, and punch-down blocks. 150m 1080p / 100m 4K60 over legacy Cat5e. At Contact RSM the cheapest insurance policy for every retrofitted install in the territory.

AVPro Edge · New
AC-EX150-BKT Contact RSM
18Gbps HDBaseT · 100m 4K60 · 150m 1080p · Splice/Coupler Tolerant

The retro install answer. The 2008 Cat5e run with a splice behind the fireplace and punch-down blocks in the attic — this extender handles it. Built to overcome exactly those inline Category wire challenges.

HDBaseT New
Must Carry
AVPro Edge
AC-EX70-444-KIT Contact RSM
18Gbps HDBaseT · 70m 4K / 150m 1080p · Full HDR · Dolby Vision · PoC · ARC · Test Pattern · Scaling

The most feature-complete standard kit. Full HDR and Dolby Vision, 4-port Ethernet pass-through, bidirectional PoC, ARC, built-in test pattern generator, and scaling. If you carry one HDBaseT kit, this is the one.

HDBaseT Full Feature
Must Carry
AVPro Edge
AC-EX40-444-KIT Contact RSM
18Gbps HDBaseT · 40m 4K / 70m 1080p · Full HDR · PoC · ARC · Test Pattern · Scaling

All the features of the 70m kit at Contact RSM less. Rack to display, closet to conference room, equipment room to ceiling projector. The standard for medium rooms.

HDBaseT 18Gbps
Must Carry
AVPro Edge
AC-EX100-444-KIT Contact RSM
18Gbps HDBaseT 3.0 · 100m 4K · USB Extension · eARC · 4-Port Ethernet · PoC

HDBaseT 3.0 for runs over 70 meters with USB pass-through and eARC. Large estate installs, commercial buildings, runs where the actual cable length is uncertain.

HDBaseT 3.0 eARC USB
Recommended
AVPro Edge
AC-EX70-UHD-ARC Contact RSM
10.2Gbps HDBaseT · 40m 4K30 / 70m 1080p · ARC · EDID · PoC

The value kit with ARC for simple residential TV runs. When 4K/30Hz covers the use case, this saves Contact RSM over the 444 kit. ARC + EDID + PoC covers most single-zone TV installs.

HDBaseT ARC
Budget Option
AVPro Edge
AC-EXUSB-3-KIT Contact RSM
USB 3.2 Gen 1 · 100m · Zoom / Teams / Logitech BRIO

USB cameras are installed AV equipment. When the Logitech BRIO run doesn't work, the conference room is dead. One of these prevents the most expensive service call: the one where a meeting gets cancelled.

USB 3.2 100m
Recommended
🔊 Audio & Dante
eARC, AEX, DAC, Dante — every audio format problem covered
AVPro Edge
AC-AEX-DEARC-KIT Contact RSM
eARC Extender Kit · 100m · Preserves Atmos/TrueHD/DTS:X

When the TV's eARC port needs to reach a processor more than a cable's length away, this extends it cleanly to 100 meters. The number-one audio service call in large residential installs — and the one-kit fix.

eARC 100m
Must Carry
AVPro Edge
AC-DAC-CO2 Contact RSM
Digital-to-Analog Converter · SPDIF/Optical → Stereo RCA

The Contact RSM fix for "there's no analog audio on this source." Optical or coax SPDIF in, clean stereo RCA out. Buy three. Leave one at every install that has a legacy amp in the chain.

DAC Contact RSM
Must Carry ×3
AVPro Edge
AC-AEX-KIT ★ Best Seller Contact RSM
100m Uncompressed Audio Extender Kit · TX + RX Included

The best-selling audio product in the line. 100 meters of uncompressed stereo audio over Cat6. Simple, fast to deploy, and the install standard for background audio zones in large homes.

Uncompressed 100m
Must Carry
AVPro Edge
AC-DANTE-E + AC-DANTE-D Contact RSM
2-Channel Dante Encoder + Decoder · Network Audio Bridge

The Dante on-ramp and off-ramp for the van. Bridge any HDMI audio source onto the Dante fabric and pull Dante audio out to any analog destination without touching installed infrastructure.

Dante 2CH
Recommended
AVPro Edge
AC-DANTE-AMP-2CH Contact RSM
2-Channel Dante Network Amplifier · 40W/ch

Pulls audio directly off the Dante network and drives speakers. No DAC, no external amp, no extra cabling. For service calls where a zone amp is down in a Dante system, this keeps the client in music.

Dante Amp
Recommended
🔌 Bullet Train Cables
Passive 18Gbps · AOC 18Gbps · Passive 48Gbps · AOC 48Gbps · USB-C
Bullet Train
AC-BTJUMP / BT01 / BT03 Contact RSM
18Gbps Passive HDMI · 0.5m / 1m / 3m · CL2/CL3 · Serial-Numbered

Short patch cables consumed constantly in the field. The BTJUMP at Contact RSM is the rack patch standard. Keep a dozen across these lengths — the backbone of every test rig, demo setup, and equipment room commissioning task.

18Gbps Patch
Must Carry ×10+
Bullet Train
AC-BT10-AUHD / AC-BT15-AUHD Contact RSM
18Gbps Passive HDMI · 10m / 15m · CL2/CL3 In-Wall Rated

10 and 15 meters cover 85% of single-room display runs without needing AOC. 18AWG conductors, serial-numbered headshells. Swap one in to verify a flaky installed run in under two minutes.

18Gbps Passive
Must Carry
Bullet Train
AC-BTSSF-5KUHD-10/20/30 Contact RSM
18Gbps 5K Active Optical · 10m / 20m / 30m · Cleerline Fiber · CL2/CL3

18Gbps AOC for runs too long for passive. EMI-immune, no signal degradation. Replace flaky passive cable without pulling a full HDBaseT system. CL2/CL3 rated — leave them in the wall.

AOC Fiber
Must Carry
Bullet Train
AC-BTSSF-10KUHD-10/15 Contact RSM
48Gbps 10K Active Optical HDMI 2.1 · 10m / 15m · Cleerline Fiber

48Gbps HDMI 2.1 AOC — 4K/120Hz, 8K/60Hz, VRR, eARC over fiber. As HDMI 2.1 displays become standard, the "projector run that only does 4K/60" failure becomes a regular complaint. These prevent it.

48Gbps HDMI 2.1
Recommended
Bullet Train
BT-USBC-01/02/03 Contact RSM
USB 3.2 Type-C to Type-C · 20Gbps · Serial-Numbered

USB-C cables that actually work. Four data lanes, 20Gbps, serial-numbered headshells. OEM cables that come with laptops are consistently the weakest link in conference room AV. Replace them once, keep them replaced.

USB-C 20Gbps
Recommended
🧪 Murideo Testing
STIX for the field · SIX-G for commissioning

The MU-STIX-G/A pair at Contact RSM is the affordable pocket tool for everyday field verification. The SIX-G is the commissioning standard for premium installs — the same tools AVPro's ISF-certified team uses. Both belong in the van.

Murideo
MU-STIX-G + MU-STIX-A Contact RSM
STIX Ecosystem Generator + Analyzer · Pocket Size

The STIX generator injects test signals at any point in the chain. The analyzer reads back what the display actually sees — EDID readout, HDR capability check, signal presence — in a form factor that fits in a shirt pocket. At Contact RSM no field tech can't justify this.

Generator Analyzer
Must Carry
Murideo
MU-SIX-G-8K-M Contact RSM
SIX-G 8K Test Pattern Generator · Full HDR Suite · Dolby Vision · Audio · HDCP 2.3

Every HDR format. Full audio test tone suite including Atmos. HDCP 2.2/2.3 handshake testing. EDID analysis. AVPro's ISF-certified team uses these. For any install you want to certify as performing as specified.

8K HDR Suite
Must Carry
Murideo
MU-SIX-A-8K-M Contact RSM
SIX-A 8K Test Pattern Analyzer · Audio Level Meter · Format ID

Audio problems are invisible. The SIX-A makes them visible — level meters, format ID, channel mapping, delay measurement. When the client says "it sounds off," the SIX-A gives you the exact data.

Analyzer Audio
Recommended
10 Years. No BS. That's the AVPro Promise.

Every product on this page carries AVPro's industry-leading 10-year manufacturer's warranty. No red tape, no asterisks. Questions on stocking, pricing, or what's right for a specific job in Northern California?

Contact Evan Dealer Program All Resources
🚐
Roll Ready Kit Builder
0 items selected · Print to generate your manifest