AV-Over-IP · The Complexity Decoder

# MXnet, Decoded

MXnet has more SKUs than any other AVPro line — 1G, 10G, USP, USB extension, multiviewer, CBOX, switches across four tiers. Four questions below resolve any project to the exact stack.

The premise MXnet has more SKUs than any other line in the AVPro Global portfolio, and the path from "I have a project" to "I have the right stack" isn't obvious. Answer four questions below, get the exact SKU list. This isn't a configurator that calls home — it's a decision tree you can use on the phone with a dealer, or in front of a client.
The Decoder · Four Questions

### 1 What are you doing?

### 2 How many displays / endpoints?

### 3 Resolution / quality requirement?

### 4 Any audio routing requirement?

Reference · The Full MXnet Line

### Switches

SKU | Tier | MSRP | Notes
--- | --- | --- | ---
AC-MXNET-SW24ENEW | 1G | $1,749 | Essential Series 24-port 1G with four 1G SFP uplinks.
AC-MXNET-SW48ENEW | 1G | $4,199 | Essential Series 48-port 1G with six 10G SFP+ uplinks.
AC-MXNET-SW48XFNEW | 10G/SDVoE | $16,799 | The big iron. 48-port 10G SFP+, 100G QSFP28 uplinks. Pro/enterprise SDVoE.
AC-MXNET-SW8P | 1G | $1,299 | Compact 1G switch. Single-zone or small system.

### USP · Universal Streaming Platform

SKU | Tier | MSRP | Notes
--- | --- | --- | ---
AC-MXNET-USP-ESNEW | USP | $899 | USP Essential. 1080p AV-over-IP TX/RX. Cost-effective unified streaming platform.
AC-MXNET-USP-PLNEW | USP | $1,299 | USP Plus. 4K60 over IP. The middle of the new USP line.
AC-MXNET-USP-PRNEW | USP | $1,699 | USP Pro. Top of the USP line. Full feature set.

### 1G Encoders / Decoders

SKU | Tier | MSRP | Notes
--- | --- | --- | ---
AC-MXNET-1G-EV2WP-B | 1G | $1,539 | 1G wallplate encoder with auto-switching HDMI inputs. Black finish.

### USB Over IP

SKU | Tier | MSRP | Notes
--- | --- | --- | ---
AC-MXNET-1G-DEX-UV2 | 1G | $599 | USB 2.0 over IP device-side RX. Pair with HEX-UV2.
AC-MXNET-1G-HEX-UV2 | 1G | $599 | USB 2.0 over IP host-side TX. For keyboard/mouse/storage extension to remote workstations.

### Multiviewer

SKU | Tier | MSRP | Notes
--- | --- | --- | ---
AC-MXNET-1G-MV41V2 | 1G | Quote | 4-input multiviewer. Picture-in-picture, quad views, video walls.

### CBOX · Controllers

SKU | Tier | MSRP | Notes
--- | --- | --- | ---
AC-MXNET-CBOX-HA | all | Quote | High-availability controller. Runs the show. Required.
AC-MXNET-DANTE-CBOX | all | Quote | CBOX variant with native Dante for audio routing alongside video.

From the Desk USP is where the line is heading. AVPro launched ES, PL, and PR (Essential, Plus, Pro) in April 2026 explicitly to retire the picking-the-right-1G-encoder problem. If your project is being designed in 2026, default to USP unless 10G SDVoE is genuinely required. The Switch + CBOX architecture is the same; you're really just picking the endpoint tier per display.